SIGHTSEEING SEMI-SUBMARINE VESSEL  
FLAG/CLASS : KOREA / KR  
PORT OF REGISTRY : PORT POHANG, KOREA  
BUILT : JULY 14, 1998, SUB-SEA SYSTEMS INC, USA  
HULL MATERIAL : ALLUMINUM ALLOY  
GRT/DWT : 40T/22T

LIGHT SHIP : 77 T  
L/B/D/DRAFT : 23.55/5.49/2.52M/1.52M  
FREEBOARD (SUMMER) : 983MM  
SPEED : 7 KNOTS  
PASSENGER : 100 PAX  
CREW : 3 P  
M/E : CATERPILLAR 3208, 150 HP X 2,100 RPM X 2 SETS  
PROPELLER : 2 SETS  
A/E : CUMMINS 68 HP  
LIFEJACKET : 108 UNITS (ADULT), 26 UNITS (CHILDREN)   
WINDOW : 3 LAYES BINDING REINFORCED GLASS, 24MM





